**How to generate a .adz file ( 7 steps)**

**Prerequisites :**

* Install 7 zip in the PC.

1) Open the DeviceFiles folder in the computer. (….\Psemi\muratastudio\DeviceFiles)

2) Select the device folder from which the .adz needs to be generated. (For eg : PE24101-102 folder). Don’t close this window.

3) Open DeviceFileCreator folder in Tools folder of your computer (…...\Psemi\muratastudio\Tools\ DeviceFileCreator).

4) Two files are present inside the DeviceFileCreator folder

* adzApplicationContainerCreator.bat – used for creating Application.adz
* adzDeviceContainerCreator.bat - used for creating devices .adz file

5) Open and place both the windows on the desktop screen ( DeviceFileCreator folder window and DeviceFiles folder window).

* Drag the selected device file into adzDeviceContainerCreator.bat to create the **PE24101-102.adz**.
* Similarly for creating **Application.adz** file, Drag the Application folder into adzApplicationContainerCreator.bat.

6) .adz files can be located in the DeviceFiles folder with the latest timestamp.

7) Copy this .adz file in to three locations given below.

* "…….\muratastudio\Apps\muRata\Devices"
* "……...\muratastudio\Apps\muRata\bin\Debug\Devices"
* "……….\muratastudio\Apps\muRata\bin\Release\Devices"